|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Month | Are all Emergency lights working with the 30 sec and 90 min functional testing? | Location of any emergency lights not working: | If repair was needed, how was it repaired? | Was it reported to Administrator? | Signature | Date |
| January |  |  |  |  |  |  |
| February |  |  |  |  |  |  |
| March |  |  |  |  |  |  |
| April |  |  |  |  |  |  |
| May |  |  |  |  |  |  |
| June |  |  |  |  |  |  |
| July |  |  |  |  |  |  |
| August |  |  |  |  |  |  |
| September |  |  |  |  |  |  |
| October |  |  |  |  |  |  |
| November |  |  |  |  |  |  |
| December |  |  |  |  |  |  |

A functional test at 30‑day intervals for not less than 30 seconds, an annual test for not less than 1‑1/2 hours must be completed and maintained written records of visual inspections and test.